General purpose one way clutch

Built-in design

AA Roller type freewheel. Outer race connection via through screws

AE Roller type freewheel. Outer race connection via press fit and/or face key

AS Roller type freewheel. Outer race connection via press fit. Mounting dimensions similar to bearing series 62 ASNU Roller type freewheel. Outer race connection via press fit and/or face key

DC Double cage sprag type freewheel. Delivered without inner and outer race

DC Races/-Ringe/Bagues DC races are offered for use with DC freewheel cages

KI Mini freewheel delivered without outer race

NF Roller type freewheel. Outer race connection via press fit and/or face key

NFR Roller type freewheel, bearing supported, without sealing. Outer race connection via press fit and/or face key

Self contained design

AL Roller type freewheel. Basic module to be completed with flange and cover

ALF2D2 Roller type freewheel. Outer race connection via screws

ALF4D2 Roller type freewheel. Outer race connection via screws

ALM Roller type freewheel. Increase torque capacity basic module to be completed with flange and cover

ALMF2D2 Roller type freewheel. Outer race connection via screws

ALMF4D2 Roller type freewheel. Outer race connection via screws

ALMPF7D7 Roller type freewheel. Outer race connection via keyway

ALP Roller type freewheel. Basic module to be completed with flange and cover. Outer race connection via keyway

ALPF7D7 Roller type freewheel. Outer race connection via keyway

ASK Bearing supported roller type freewheel. Mounting dimensions as ball bearing series 60

CSK Bearing/freewheel. Dimensions identical to ball bearing series 62

CSK2RS Sealed bearing/freewheel. Diameters identical to ball bearing series 62

CSKP Bearing/freewheel. Dimensions identical to ball bearing series 62… Keyway in inner race

CSKP2RS Bearing/freewheel. Diameters identical to ball bearing series 62… Keyway in inner race

CSKPP Bearing/freewheel. Dimensions identical to ball bearing series 62… Keyway in inner and outer race

FS 750-1027 Sprag type freewheel to USA standard. Outer race connection via face screws

FSO 300-700 Sprag type freewheel to USA standard. Outer race connection via face screws

FSO 300-700 GR Sprag type freewheel to USA standard. Outer race connection via face screws

FSO 750-1027 Sprag type freewheel to USA standard. Outer race connection via face screws

GFK Bearing/freewheel. Dimensions identical to ball bearing series 59

GFR Roller type freewheel. Basic module to be completed with flange and cover

GFRF1F2 Roller type freewheel. Outer race connection made via face screws

GFRF2F7 Roller type freewheel. Outer race connection made via face screws

GFRN Roller type freewheel. Basic module to be completed with flange and cover. Outer race connection via keyway

GFRNF5F6 Roller type freewheel. Outer race connection via keyway

SMZ Bearing supported sprag type. Grease lubricated. Connection outer race with face screws

Indexing clutch

BAT Single revolution clutch. Cage driven roller type freewheel

HPI 300-700 Sprag type freewheel to USA standard. Outer race connection via face screws

HPI 750-1027 Sprag type freewheel to USA standard. Outer race connection via face screws

Backstop

Built-in design

CR Centrifugal lift off sprag type freewheel. To be used only for replacement

RSBF Centrifugal lift off sprag type freewheel. To be used only for replacement

RSBI Centrifugal lift off sprag type freewheel. To be used only for replacement

RSCI Centrifugal lift off sprag type freewheel when the inner race rotates

Self contained design

AV Roller type freewheel for low speed. Outer race connection via torque arm

GFRF2F3 Roller type freewheel. Outer race connection via torque arm

GFRF3F4 Roller type freewheel. Outer race connection via torque arm

RIZG2G3 Centrifugal lift off sprag type freewheel for high speed. Outer race connection via torque arm

RIZG3G4 Centrifugal lift off sprag type freewheel for high speed. Outer race connection via torque arm

RSBW Sprag type freewheel for low speed. Outer race connection via torque arm

Overrunning clutch

Built-in design

RSBI Centrifugal lift off sprag type freewheel. To be used only for replacement

RSCI Centrifugal lift off sprag type freewheel when the inner race rotates

Self contained design

ALG Encased freewheel for high speed

ALKEED2 Roller type freewheel with highly elastic coupling

ALKMSD2 Roller type freewheel with elastic coupling

ALMKEED2 Roller type freewheel with highly elastic coupling

ALMKMSD2 Roller type freewheel with elastic coupling

RIZ Centrifugal lift off sprag type freewheel. Basic module to be completed with flange and cover

RIZELG2 Centrifugal lift off sprag type freewheel with highly elastic coupling

RIZESG2 Centrifugal lift off sprag type freewheel with elastic coupling

RIZG1G2 Centrifugal lift off sprag type freewheel. Outer race connection via screws

RIZG2G7 Centrifugal lift off sprag type freewheel. Outer race connection via face screws